{"text_format":"1","workbook":"xlsx","n_sheets":11,"sheets":["流出係数算出","降雨強度","流入量定義","01流出計算（Q-Tグラフ）","浸透施設能力","浸透施設能力（貯留浸透モデル_道路管理者用）","02流出計算（QT-Sグラフ）","03-①調整池容量の概算","04-①調節計算（自然調節方式）","04-②調節計算（2段）","04-③調節計算（ポンプ）"],"not_rendered":{"charts":5,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"流出係数算出","index":0,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[[7,1,7,4],[26,1,30,3],[1,4,2,5],[23,2,25,3],[18,1,25,1],[8,1,17,1],[4,1,4,7],[18,2,19,3],[8,2,17,3],[6,1,6,3],[20,2,22,3]]}
[null,null,null,null,null,null,null,null,"行為前Σan","行為後Σan"]
[null,null,null,null,"流出係数算定結果",null,"行為前","行為後",{"$f":"SUM($G$9:$G$95)","v":0},{"$f":"SUM($H$9:$H$95)","v":0}]
[null,null,null,null,null,null,{"$f":"$I$4/$I$2","v":{"$error":"#DIV/0!"}},{"$f":"$J$4/$J$2","v":{"$error":"#DIV/0!"}},"行為前Σ(fn*an)","行為後Σ(fn*an)"]
[null,null,null,null,null,null,null,null,{"$f":"SUM($I$9:$I$95)","v":0},{"$f":"SUM($J$9:$J$95)","v":0}]
[null,"雨水浸透阻害行為の技術基準として設定する流出係数"]
[]
[null,"区分",null,null,"土地利用の形態の細区分","流出係数","行為前面積\n（ha）","行為後面積\n（ha）"]
[null,"計",null,null,null,"－",{"$f":"SUM(G9:G31)","v":0},{"$f":"SUM(H9:H31)","v":0}]
[null,"宅地等に該当する土地","第１号関連",null,"宅地",0.9,null,null,{"$f":"$F9*$G9","v":0},{"$f":"$F9*$H9","v":0}]
[null,null,null,null,"池沼",1,null,null,0,0]
[null,null,null,null,"水路",1,null,null,0,0]
[null,null,null,null,"ため池",1,null,null,0,0]
[null,null,null,null,"道路(法面を有しないもの）",0.9,null,null,0,0]
[null,null,null,null,"道路（法面を有するもの）",null,null,null,0,0]
[null,null,null,null,"鉄道線路（法面を有しないもの）",0.9,null,null,0,0]
[null,null,null,null,"鉄道線路（法面を有するもの）",null,null,null,0,0]
[null,null,null,null,"飛行場（法面を有しないもの）",0.9,null,null,0,0]
[null,null,null,null,"飛行場（法面を有するもの）",null,null,null,0,0]
[null,"宅地等以外の土地","第２号\n関　連",null,"不浸透性材料により舗装された土地（法面を除く）",0.95,null,null,0,0]
[null,null,null,null,"不浸透性材料により覆われた法面",1,null,null,0,0]
[null,null,"第３号\n関　連",null,"ゴルフ場（雨水を排除するための排水施設を伴うものに限る）",0.5,null,null,0,0]
[null,null,null,null,"運動場その他これに類する施設（雨水を排除するための排水施設を伴うものに限る）",0.8,null,null,0,0]
[null,null,null,null,"ローラーその他これに類する建設機械を用いて締め固められた土地",0.5,null,null,0,0]
[null,null,"上記第１号から第３号に掲げる土地以外の土地",null,"山地",0.3,null,null,0,0]
[null,null,null,null,"人工的に造成され植生に覆われた法面",0.4,null,null,0,0]
[null,null,null,null,"林地、耕地、原野その他ローラーその他これに類する建設機械を用いて締め固められていない土地",0.2,null,null,{"$f":"$F26*$G26","v":0},0]
[null,"そ\n\n\nの\n\n\n他",null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,null,null,null,null,0,0]

{"sheet":"降雨強度","index":1,"n_rows":38,"n_cols":12,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
["※降雨は対象地域の降雨に変更して下さい"]
["時","分","降雨量\n（mm/h）","時","分","降雨量\n（mm/h）","時","分","降雨量\n（mm/h）","時","分","降雨量\n（mm/h）"]
[0,"0－10",2.2999999999999998,6,"0－10",4,12,"0－10",69.2,18,"0－10",3.9]
[null,"10－20",2.2999999999999998,null,"10－20",4.0999999999999996,null,"10－20",42.8,null,"10－20",3.8]
[null,"20－30",2.2999999999999998,null,"20－30",4.2,null,"20－30",31.5,null,"20－30",3.7]
[null,"30－40",2.2999999999999998,null,"30－40",4.3,null,"30－40",25.1,null,"30－40",3.6]
[null,"40－50",2.4,null,"40－50",4.4000000000000004,null,"40－50",20.9,null,"40－50",3.6]
[null,"50－60",2.4,null,"50－60",4.5,null,"50－60",18,null,"50－60",3.5]
[1,"0－10",2.4,7,"0－10",4.7,13,"0－10",15.8,19,"0－10",3.4]
[null,"10－20",2.5,null,"10－20",4.8,null,"10－20",14.1,null,"10－20",3.4]
[null,"20－30",2.5,null,"20－30",5,null,"20－30",12.8,null,"20－30",3.3]
[null,"30－40",2.5,null,"30－40",5.0999999999999996,null,"30－40",11.7,null,"30－40",3.2]
[null,"40－50",2.5,null,"40－50",5.3,null,"40－50",10.8,null,"40－50",3.2]
[null,"50－60",2.6,null,"50－60",5.5,null,"50－60",10,null,"50－60",3.1]
[2,"0－10",2.6,8,"0－10",5.7,14,"0－10",9.3000000000000007,20,"0－10",3.1]
[null,"10－20",2.7,null,"10－20",5.9,null,"10－20",8.8000000000000007,null,"10－20",3]
[null,"20－30",2.7,null,"20－30",6.1,null,"20－30",8.3000000000000007,null,"20－30",3]
[null,"30－40",2.7,null,"30－40",6.3,null,"30－40",7.8,null,"30－40",2.9]
[null,"40－50",2.8,null,"40－50",6.6,null,"40－50",7.4,null,"40－50",2.9]
[null,"50－60",2.8,null,"50－60",6.9,null,"50－60",7.1,null,"50－60",2.8]
[3,"0－10",2.9,9,"0－10",7.3,15,"0－10",6.8,21,"0－10",2.8]
[null,"10－20",2.9,null,"10－20",7.6,null,"10－20",6.5,null,"10－20",2.8]
[null,"20－30",2.9,null,"20－30",8,null,"20－30",6.2,null,"20－30",2.7]
[null,"30－40",3,null,"30－40",8.5,null,"30－40",6,null,"30－40",2.7]
[null,"40－50",3,null,"40－50",9,null,"40－50",5.8,null,"40－50",2.6]
[null,"50－60",3.1,null,"50－60",9.6999999999999993,null,"50－60",5.6,null,"50－60",2.6]
[4,"0－10",3.1,10,"0－10",10.4,16,"0－10",5.4,22,"0－10",2.6]
[null,"10－20",3.2,null,"10－20",11.2,null,"10－20",5.2,null,"10－20",2.5]
[null,"20－30",3.3,null,"20－30",12.2,null,"20－30",5,null,"20－30",2.5]
[null,"30－40",3.3,null,"30－40",13.4,null,"30－40",4.9000000000000004,null,"30－40",2.5]
[null,"40－50",3.4,null,"40－50",14.9,null,"40－50",4.7,null,"40－50",2.4]
[null,"50－60",3.4,null,"50－60",16.8,null,"50－60",4.5999999999999996,null,"50－60",2.4]
[5,"0－10",3.5,11,"0－10",19.3,17,"0－10",4.5,23,"0－10",2.4]
[null,"10－20",3.6,null,"10－20",22.8,null,"10－20",4.4000000000000004,null,"10－20",2.2999999999999998]
[null,"20－30",3.7,null,"20－30",27.9,null,"20－30",4.3,null,"20－30",2.2999999999999998]
[null,"30－40",3.7,null,"30－40",36.200000000000003,null,"30－40",4.0999999999999996,null,"30－40",2.2999999999999998]
[null,"40－50",3.8,null,"40－50",52.7,null,"40－50",4.0999999999999996,null,"40－50",2.2999999999999998]
[null,"50－60",3.9,null,"50－60",106.8,null,"50－60",4,null,"50－60",2.2000000000000002]

{"sheet":"流入量定義","index":2,"n_rows":147,"n_cols":2,"rows_kept":147,"cut":false,"hidden":false,"merged":[]}
["※流出計算を実行する場合、記入する必要はありません。"]
["時刻","行為後流入量"]
["00:00:00"]
["00:10:00",0]
["00:20:00",6.9999999999999999E-4]
["00:30:00",7.2000000000000005E-4]
["00:40:00",7.2000000000000005E-4]
["00:50:00",7.2000000000000005E-4]
["01:00:00",7.5000000000000002E-4]
["01:10:00",7.5000000000000002E-4]
["01:20:00",7.5000000000000002E-4]
["01:30:00",7.7999999999999999E-4]
["01:40:00",7.7999999999999999E-4]
["01:50:00",7.7999999999999999E-4]
["02:00:00",8.0000000000000004E-4]
["02:10:00",8.0000000000000004E-4]
["02:20:00",8.1999999999999998E-4]
["02:30:00",8.1999999999999998E-4]
["02:40:00",8.1999999999999998E-4]
["02:50:00",8.4999999999999995E-4]
["03:00:00",8.4999999999999995E-4]
["03:10:00",8.8000000000000003E-4]
["03:20:00",8.8000000000000003E-4]
["03:30:00",8.9999999999999998E-4]
["03:40:00",8.9999999999999998E-4]
["03:50:00",9.3000000000000005E-4]
["04:00:00",9.3000000000000005E-4]
["04:10:00",9.5E-4]
["04:20:00",9.7000000000000005E-4]
["04:30:00",9.7000000000000005E-4]
["04:40:00",1E-3]
["04:50:00",1E-3]
["05:00:00",1.0200000000000001E-3]
["05:10:00",1.0499999999999999E-3]
["05:20:00",1.07E-3]
["05:30:00",1.07E-3]
["05:40:00",1.1000000000000001E-3]
["05:50:00",1.1299999999999999E-3]
["06:00:00",1.15E-3]
["06:10:00",1.1800000000000001E-3]
["06:20:00",1.1999999999999999E-3]
["06:30:00",1.23E-3]
["06:40:00",1.25E-3]
["06:50:00",1.2800000000000001E-3]
["07:00:00",1.2999999999999999E-3]
["07:10:00",1.3500000000000001E-3]
["07:20:00",1.3799999999999999E-3]
["07:30:00",1.4E-3]
["07:40:00",1.4499999999999999E-3]
["07:50:00",1.5E-3]
["08:00:00",1.5200000000000001E-3]
["08:10:00",1.58E-3]
["08:20:00",1.6299999999999999E-3]
["08:30:00",1.6800000000000001E-3]
["08:40:00",1.75E-3]
["08:50:00",1.8E-3]
["09:00:00",1.8799999999999999E-3]
["09:10:00",1.9499999999999999E-3]
["09:20:00",2.0500000000000002E-3]
["09:30:00",2.1299999999999999E-3]
["09:40:00",2.2499999999999998E-3]
["09:50:00",2.3500000000000001E-3]
["10:00:00",2.47E-3]
["10:10:00",2.65E-3]
["10:20:00",2.8E-3]
["10:30:00",3.0300000000000001E-3]
["10:40:00",3.2499999999999999E-3]
["10:50:00",3.5500000000000002E-3]
["11:00:00",3.8999999999999998E-3]
["11:10:00",4.3499999999999997E-3]
["11:20:00",4.9500000000000004E-3]
["11:30:00",5.7800000000000004E-3]
["11:40:00",6.9800000000000001E-3]
["11:50:00",8.9800000000000001E-3]
["12:00:00",1.3050000000000001E-2]
["12:10:00",2.9000000000000001E-2]
["12:20:00",1.7399999999999999E-2]
["12:30:00",1.06E-2]
["12:40:00",7.8499999999999993E-3]
["12:50:00",6.3299999999999997E-3]
["13:00:00",5.3299999999999997E-3]
["13:10:00",4.62E-3]
["13:20:00",4.13E-3]
["13:30:00",3.7200000000000002E-3]
["13:40:00",3.3999999999999998E-3]
["13:50:00",3.13E-3]
["14:00:00",2.8999999999999998E-3]
["14:10:00",2.7299999999999998E-3]
["14:20:00",2.5500000000000002E-3]
["14:30:00",2.4299999999999999E-3]
["14:40:00",2.3E-3]
["14:50:00",2.1700000000000001E-3]
["15:00:00",2.0799999999999998E-3]
["15:10:00",2E-3]
["15:20:00",1.92E-3]
["15:30:00",1.8500000000000001E-3]
["15:40:00",1.7700000000000001E-3]
["15:50:00",1.73E-3]
["16:00:00",1.65E-3]
["16:10:00",1.6000000000000001E-3]
["16:20:00",1.5499999999999999E-3]
["16:30:00",1.5E-3]
["16:40:00",1.48E-3]
["16:50:00",1.4300000000000001E-3]
["17:00:00",1.4E-3]
["17:10:00",1.3500000000000001E-3]
["17:20:00",1.32E-3]
["17:30:00",1.2999999999999999E-3]
["17:40:00",1.2800000000000001E-3]
["17:50:00",1.23E-3]
["18:00:00",1.1999999999999999E-3]
["18:10:00",1.1800000000000001E-3]
["18:20:00",1.15E-3]
["18:30:00",1.1299999999999999E-3]
["18:40:00",1.1299999999999999E-3]
["18:50:00",1.1000000000000001E-3]
["19:00:00",1.07E-3]
["19:10:00",1.0499999999999999E-3]
["19:20:00",1.0200000000000001E-3]
["19:30:00",1.0200000000000001E-3]
["19:40:00",1E-3]
["19:50:00",9.7000000000000005E-4]
["20:00:00",9.7000000000000005E-4]
["20:10:00",9.5E-4]
["20:20:00",9.5E-4]
["20:30:00",9.3000000000000005E-4]
["20:40:00",9.3000000000000005E-4]
["20:50:00",8.9999999999999998E-4]
["21:00:00",8.9999999999999998E-4]
["21:10:00",8.8000000000000003E-4]
["21:20:00",8.8000000000000003E-4]
["21:30:00",8.4999999999999995E-4]
["21:40:00",8.4999999999999995E-4]
["21:50:00",8.1999999999999998E-4]
["22:00:00",8.1999999999999998E-4]
["22:10:00",8.0000000000000004E-4]
["22:20:00",8.0000000000000004E-4]
["22:30:00",8.0000000000000004E-4]
["22:40:00",7.7999999999999999E-4]
["22:50:00",7.7999999999999999E-4]
["23:00:00",7.7999999999999999E-4]
["23:10:00",7.5000000000000002E-4]
["23:20:00",7.5000000000000002E-4]
["23:30:00",7.5000000000000002E-4]
["23:40:00",7.2000000000000005E-4]
["23:50:00",7.2000000000000005E-4]
["24:00",0]

{"sheet":"01流出計算（Q-Tグラフ）","index":3,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,1,1,5],[1,7,1,24],[22,2,24,4],[9,2,12,4],[17,2,18,5]]}
[]
[null,"流 出 計 算 条 件",null,null,null,null,null,"流 出 計 算 結 果"]
[]
[null,null,null,null,null,null,null,"時刻","行為前流入量","行為後流入量","降雨強度"]
[null,1,"流出計算の実行"]
[]
[null,null,"行為面積",{"$f":"流出係数算出!$H$8","v":0},"ha"]
[]
[null,null,"降雨量"]
[null,null,"※「降雨強度」シートに基準降雨を入力してください。（都道府県知事等により公示されている「基準降雨」の値に変更してください。）"]
[]
[]
[]
[]
[null,null,"流出係数"]
[null,null,"行為前",{"$error":"#DIV/0!"}]
[null,null,"行為後",{"$error":"#DIV/0!"}]
[null,null,"※「流出係数算出」シートで算出した諸元が入力されていますが、必要に応じて申請図書記載値に上書きすることができます。"]
[]
[]
[null,null,"流出計算結果の指定"]
[]
[null,null,"※「流入量定義」シートに計算された流出計算結果（行為後）を入力してください。"]
[]
[]
[]
[null,null,"許容放流量",0.01,"m3/s"]

{"sheet":"浸透施設能力","index":4,"n_rows":62,"n_cols":19,"rows_kept":62,"cut":false,"hidden":false,"merged":[[49,1,51,1],[49,2,49,3],[49,4,51,4],[49,5,49,7],[49,12,51,12],[50,2,51,2],[50,3,51,3],[49,13,51,13],[49,14,51,14],[21,13,23,13],[21,14,23,14],[22,3,23,3],[21,12,23,12],[35,14,37,14],[35,13,37,13],[35,12,37,12],[36,3,37,3],[21,1,23,1],[21,2,21,3],[21,4,23,4],[21,5,21,7],[35,1,37,1],[35,2,35,3],[35,4,37,4],[35,5,35,7],[22,2,23,2],[36,2,37,2],[3,2,3,3],[3,13,3,14],[7,1,9,1],[7,2,7,3],[7,4,9,4],[7,5,7,7],[7,12,9,12],[7,13,9,13],[7,14,9,14],[8,2,9,2],[8,3,9,3],[1,1,1,6],[1,12,1,17],[2,2,2,3],[2,6,2,7],[2,13,2,14],[2,17,2,18]]}
[]
[null,"浸透施設能力算定結果",null,null,null,null,null,null,null,null,null,null,"空隙貯留量算定結果"]
[null,"浸透マス","浸透トレンチ",null,"透水性舗装","その他","浸透施設能力算定結果",null,null,null,null,null,"浸透マス","浸透トレンチ",null,"透水性舗装","その他","空隙貯留量算定結果"]
[null,{"$f":"SUM(I11:J20)","v":0},{"$f":"SUM(J25:J34)","v":0},null,{"$f":"SUM(J39:J48)","v":0},{"$f":"SUM(J53:J62)","v":0},{"$f":"B4+C4+E4+F4","v":0},"ｍ3/ｈｒ",null,null,null,null,{"$f":"SUM(K11:K20)/100","v":0},{"$f":"SUM(K25:K34)/100","v":0},null,{"$f":"SUM(K39:K48)/100","v":0},{"$f":"SUM(K53:K62)/100","v":0},{"$f":"M4+N4+P4+Q4","v":0},"ｍ3"]
[null,null,null,null,null,null,{"$f":"G4/3600","v":0},"ｍ3/s"]
[]
[null,"条件設定",null,null,null,null,null,null,null,null,null,null,"条件設定"]
[null,"【浸透マス】","単位設計浸透能（ｍ3/ｈｒ/個）",null,"設置数量\n（個）","影響係数",null,null,null,null,null,null,"【浸透マス】","体積\n（ｍ3）","空隙率\n（％）"]
[null,null,"比浸透量（㎡）","飽和透水係数\n（m/hr）",null,"（1）","（2）","（3）"]
[null,null,null,null,null,"内容（１）","内容（２）","内容（３）"]
[null,1,null,null,null,1,1,1,null,{"$f":"$C11*$D11*$E11*$F11*$G11*$H11","v":0},{"$f":"$N11*O11","v":0},null,1]
[null,2,null,null,null,1,1,1,null,{"$f":"$C12*$D12*$E12*$F12*$G12*$H12","v":0},{"$f":"$N12*O12","v":0},null,2]
[null,3,null,null,null,1,1,1,null,0,0,null,3]
[null,4,null,null,null,1,1,1,null,0,0,null,4]
[null,5,null,null,null,1,1,1,null,0,0,null,5]
[null,6,null,null,null,1,1,1,null,0,0,null,6]
[null,7,null,null,null,1,1,1,null,0,0,null,7]
[null,8,null,null,null,1,1,1,null,0,0,null,8]
[null,9,null,null,null,1,1,1,null,0,0,null,9]
[null,10,null,null,null,1,1,1,null,0,0,null,10]
[]
[null,"【浸透トレンチ】","単位設計浸透能（ｍ3/ｈｒ/m）",null,"設置数量\n（ｍ）","影響係数",null,null,null,null,null,null,"【浸透トレンチ】","体積\n（ｍ3）","空隙率\n（％）"]
[null,null,"比浸透量（㎡）","飽和透水係数\n（m/hr）",null,"（1）","（2）","（3）"]
[null,null,null,null,null,"内容（１）","内容（２）","内容（３）"]
[null,1,null,null,null,1,1,1,null,{"$f":"$C25*$D25*$E25*$F25*$G25*$H25","v":0},{"$f":"$N25*O25","v":0},null,1]
[null,2,null,null,null,1,1,1,null,{"$f":"$C26*$D26*$E26*$F26*$G26*$H26","v":0},0,null,2]
[null,3,null,null,null,1,1,1,null,0,0,null,3]
[null,4,null,null,null,1,1,1,null,0,0,null,4]
[null,5,null,null,null,1,1,1,null,0,0,null,5]
[null,6,null,null,null,1,1,1,null,0,0,null,6]
[null,7,null,null,null,1,1,1,null,0,0,null,7]
[null,8,null,null,null,1,1,1,null,0,0,null,8]
[null,9,null,null,null,1,1,1,null,0,0,null,9]
[null,10,null,null,null,1,1,1,null,0,0,null,10]
[]
[null,"【透水性舗装】","単位設計浸透能（ｍ3/ｈｒ/㎡）",null,"設置数量\n（㎡）","影響係数",null,null,null,null,null,null,"【透水性塗装】","体積\n（ｍ3）","空隙率\n（％）"]
[null,null,"比浸透量（㎡）","飽和透水係数\n（m/hr）",null,"（1）","（2）","（3）"]
[null,null,null,null,null,"内容（１）","内容（２）","内容（３）"]
[null,1,null,null,null,1,1,1,null,{"$f":"$C39*$D39*$E39*$F39*$G39*$H39","v":0},{"$f":"$N39*O39","v":0},null,1]
[null,2,null,null,null,1,1,1,null,{"$f":"$C40*$D40*$E40*$F40*$G40*$H40","v":0},{"$f":"$N40*O40","v":0},null,2]
[null,3,null,null,null,1,1,1,null,0,0,null,3]
[null,4,null,null,null,1,1,1,null,0,0,null,4]
[null,5,null,null,null,1,1,1,null,0,0,null,5]
[null,6,null,null,null,1,1,1,null,0,0,null,6]
[null,7,null,null,null,1,1,1,null,0,0,null,7]
[null,8,null,null,null,1,1,1,null,0,0,null,8]
[null,9,null,null,null,1,1,1,null,0,0,null,9]
[null,10,null,null,null,1,1,1,null,0,0,null,10]
[]
[null,"【その他】","単位設計浸透能（ｍ3/ｈｒ/単位）",null,"設置数量\n（単位）","影響係数",null,null,null,null,null,null,"【その他】","体積\n（ｍ3）","空隙率\n（％）"]
[null,null,"比浸透量（㎡）","飽和透水係数\n（m/hr）",null,"（1）","（2）","（3）"]
[null,null,null,null,null,"内容（１）","内容（２）","内容（３）"]
[null,1,null,null,null,1,1,1,null,{"$f":"$C53*$D53*$E53*$F53*$G53*$H53","v":0},{"$f":"$N53*O53","v":0},null,1]
[null,2,null,null,null,1,1,1,null,0,0,null,2]
[null,3,null,null,null,1,1,1,null,0,0,null,3]
[null,4,null,null,null,1,1,1,null,0,0,null,4]
[null,5,null,null,null,1,1,1,null,0,0,null,5]
[null,6,null,null,null,1,1,1,null,0,0,null,6]
[null,7,null,null,null,1,1,1,null,0,0,null,7]
[null,8,null,null,null,1,1,1,null,0,0,null,8]
[null,9,null,null,null,1,1,1,null,0,0,null,9]
[null,10,null,null,null,1,1,1,null,0,0,null,10]

{"sheet":"浸透施設能力（貯留浸透モデル_道路管理者用）","index":5,"n_rows":58,"n_cols":19,"rows_kept":58,"cut":false,"hidden":false,"merged":[[53,1,53,2],[54,1,54,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[52,1,52,2],[37,10,39,10],[37,11,39,11],[37,12,39,12],[52,6,52,7],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[38,7,39,7],[38,8,39,8],[37,5,39,5],[37,6,39,6],[37,7,37,8],[29,1,29,2],[30,1,30,2],[31,1,31,2],[38,3,39,3],[38,4,39,4],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[37,1,39,2],[37,3,37,4],[23,18,25,18],[24,3,25,3],[24,4,25,4],[24,7,25,7],[24,8,25,8],[23,16,25,16],[23,17,25,17],[23,10,25,10],[23,11,25,11],[23,12,25,12],[23,15,25,15],[23,7,23,8],[27,1,27,2],[28,1,28,2],[21,1,21,6],[23,1,25,2],[23,3,23,4],[23,5,25,5],[23,6,25,6],[26,1,26,2],[16,1,16,2],[16,9,16,10],[17,1,17,2],[17,9,17,10],[18,1,18,2],[18,9,18,10],[15,1,15,2],[15,9,15,10],[8,1,9,1],[8,6,8,7],[9,6,9,7],[10,1,10,6],[11,1,11,3],[12,1,12,2],[12,9,12,10],[13,1,13,2],[13,9,13,10],[14,1,14,2],[14,9,14,10],[6,1,7,1],[6,6,6,7],[7,6,7,7],[1,7,1,8],[2,1,2,6],[4,1,4,2],[5,1,5,2],[5,6,5,7]]}
[]
["透水性舗装",null,null,null,null,null,null,"部分を入力して下さい"]
[]
[null,"基本諸元"]
[null,"設置数量(舗装面積) (m2)",null,3000]
[null,"飽和透水係数 （m/hr）",null,7.1999999999999998E-3,null,null,"上層路盤での貯留率(%)",null,{"$f":"L17","v":12.5}]
[null,"比浸透量算定定数\nK=aH+b","a",1.4E-2,null,null,"下層路盤での貯留率(%)",null,{"$f":"L18","v":4.5}]
[null,null,"b",1.2869999999999999,null,null,"下層路盤厚(mm)",null,{"$f":"D18","v":400}]
[null,"目詰まり\n係数","C1",0.9,null,null,"下層路盤での貯留量(mm)",null,{"$f":"M18","v":18}]
[null,null,"C2",0.9,null,null,"貯留量の合計(mm)",null,{"$f":"M19","v":55.5}]
[]
[null,"貯留率と水拘束率"]
[null,null,null,"厚さ(mm)","空気間隙率\n(%)","空気間隙率との関係","水拘束率\n(%)","水拘束量\n(mm)","貯留率\n(%)","貯留量\n(mm)",null,"STEP2での\n貯留率\n(%)","STEP2での\n貯留量\n(mm)"]
[null,"関係式",null,"a","b","b'","c","a×c/100","d (=b+b')","a×d/100",null,"d-c","a×(d-c)/100"]
[null,"表層",null,50,20,-6,1.5,{"$f":"D15*G15/100","v":0.75},{"$f":"E15+F15","v":14},{"$f":"D15*I15/100","v":7},null,{"$f":"I15-G15","v":12.5},{"$f":"D15*(I15-G15)/100","v":6.25}]
[null,"中間層・基層",null,100,20,-6,1.5,{"$f":"D16*G16/100","v":1.5},{"$f":"E16+F16","v":14},{"$f":"D16*I16/100","v":14},null,{"$f":"I16-G16","v":12.5},{"$f":"D16*(I16-G16)/100","v":12.5}]
[null,"上層路盤",null,150,20,-6,1.5,{"$f":"D17*G17/100","v":2.25},{"$f":"E17+F17","v":14},{"$f":"D17*I17/100","v":21},null,{"$f":"I17-G17","v":12.5},{"$f":"D17*(I17-G17)/100","v":18.75}]
[null,"下層路盤",null,400,8,-3,0.5,{"$f":"D18*G18/100","v":2},{"$f":"E18+F18","v":5},{"$f":"D18*I18/100","v":20},null,{"$f":"I18-G18","v":4.5},{"$f":"D18*(I18-G18)/100","v":18}]
[null,"合計",null,{"$f":"SUM(D15:D18)","v":700},"-","-","-",{"$f":"SUM(H15:H18)","v":6.5},"-",{"$f":"SUM(J15:J18)","v":62},null,"-",{"$f":"SUM(M15:M18)","v":55.5}]
[]
["浸透マス・トレンチ"]
[]
[null,"浸透能諸元",null,null,null,null,null,null,null,null,"空隙貯留諸元"]
[null,"【浸透マス】",null,"単位設計浸透能（ｍ3/ｈｒ/個）",null,"設置数量\n（個）","設計水頭\n(m)","影響係数",null,null,"【浸透\nマス】","体積\n（ｍ3）","空隙率\n（％）",null,null,"Σ","設計浸透量","平均設計水頭","設計空隙貯留量"]
[null,null,null,"比浸透量（㎡）","飽和透水係数\n（m/hr）",null,null,"地下水位\n係数","目詰まり\n係数"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"小計"]
[null,1,null,10,7.1999999999999998E-3,10,0.8,1,1,null,1,500,20,null,null,{"$f":"D27*E27*F27*G27*H27*I27","v":0.57599999999999996},{"$f":"D27*E27*F27*H27*I27","v":0.72},null,{"$f":"L27*M27/100","v":100}]
[null,2,null,null,null,null,null,1,1,null,2,null,null,null,null,{"$f":"D28*E28*F28*G28*H28*I28","v":0},{"$f":"D28*E28*F28*H28*I28","v":0},null,{"$f":"L28*M28/100","v":0}]
[null,3,null,null,null,null,null,1,1,null,3,null,null,null,null,0,0,null,0]
[null,4,null,null,null,null,null,1,1,null,4,null,null,null,null,0,0,null,0]
[null,5,null,null,null,null,null,1,1,null,5,null,null,null,null,0,0,null,0]
[null,6,null,null,null,null,null,1,1,null,6,null,null,null,null,0,0,null,0]
[null,7,null,null,null,null,null,1,1,null,7,null,null,null,null,0,0,null,0]
[null,8,null,null,null,null,null,1,1,null,8,null,null,null,null,0,0,null,0]
[null,9,null,null,null,null,null,1,1,null,9,null,null,null,null,0,0,null,0]
[null,10,null,null,null,null,null,1,1,null,10,null,null,null,null,0,0,null,0]
[]
[null,"【浸透トレンチ】",null,"単位設計浸透能（ｍ3/ｈｒ/m）",null,"設置数量\n（ｍ）","設計水頭\n(m)","影響係数",null,null,"【浸透\nトレンチ】","体積\n（ｍ3）","空隙率\n（％）"]
[null,null,null,"比浸透量（㎡）","飽和透水係数\n（m/hr）",null,null,"地下水位\n係数","目詰まり\n係数"]
[]
[null,1,null,null,null,null,null,1,1,null,1,null,null,null,null,{"$f":"D41*E41*F41*G41*H41*I41","v":0},{"$f":"D41*E41*F41*H41*I41","v":0},null,{"$f":"L41*M41/100","v":0}]
[null,2,null,null,null,null,null,1,1,null,2,null,null,null,null,{"$f":"D42*E42*F42*G42*H42*I42","v":0},{"$f":"D42*E42*F42*H42*I42","v":0},null,0]
[null,3,null,null,null,null,null,1,1,null,3,null,null,null,null,0,0,null,0]
[null,4,null,null,null,null,null,1,1,null,4,null,null,null,null,0,0,null,0]
[null,5,null,null,null,null,null,1,1,null,5,null,null,null,null,0,0,null,0]
[null,6,null,null,null,null,null,1,1,null,6,null,null,null,null,0,0,null,0]
[null,7,null,null,null,null,null,1,1,null,7,null,null,null,null,0,0,null,0]
[null,8,null,null,null,null,null,1,1,null,8,null,null,null,null,0,0,null,0]
[null,9,null,null,null,null,null,1,1,null,9,null,null,null,null,0,0,null,0]
[null,10,null,null,null,null,null,1,1,null,10,null,null,null,null,0,0,null,0]
[]
[null,"統合諸元"]
[null,"設計浸透能(m3/hr)",null,{"$f":"Q55","v":0.72}]
[null,"平均設計水頭(m)",null,{"$f":"IF(D53>0,+R55,0)","v":0.79999999999999993}]
[null,"設計空隙貯留量(m3)",null,{"$f":"S55","v":100},null,null,null,null,null,null,null,null,null,null,"総合計",{"$f":"P57+P58","v":0.57599999999999996},{"$f":"Q57+Q58","v":0.72},{"$f":"P55/Q55","v":0.79999999999999993},{"$f":"S57+S58","v":100}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"マス",{"$f":"SUM(P27:P36)","v":0.57599999999999996},{"$f":"SUM(Q27:Q36)","v":0.72},{"$f":"P57/Q57","v":0.79999999999999993},{"$f":"SUM(S27:S36)","v":100}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"トレンチ",{"$f":"SUM(P41:P50)","v":0},{"$f":"SUM(Q41:Q50)","v":0},{"$f":"P58/Q58","v":{"$error":"#DIV/0!"}},{"$f":"SUM(S41:S50)","v":0}]

{"sheet":"02流出計算（QT-Sグラフ）","index":6,"n_rows":13,"n_cols":10,"rows_kept":13,"cut":false,"hidden":false,"merged":[[7,2,8,5],[12,2,14,5],[1,1,1,5],[1,7,1,23]]}
[]
[null,"流 出 計 算 条 件",null,null,null,null,null,"流 出 計 算 結 果"]
[]
[null,null,null,null,null,null,null,"時刻","浸透考慮前","浸透考慮後"]
[null,1,"浸透施設なし"]
[]
[null,null,"浸透施設あり"]
[null,null,"※「浸透施設能力」シートに浸透施設諸元を入力してください。"]
[]
[]
[null,null,"浸透施設あり"]
[null,null,"（貯留浸透モデル_道路管理者用）"]
[null,null,"※「浸透施設能力（貯留浸透モデル_道路管理者用）」シートに浸透施設諸元を入力してください。"]

{"sheet":"03-①調整池容量の概算","index":7,"n_rows":14,"n_cols":12,"rows_kept":14,"cut":false,"hidden":false,"merged":[[13,3,13,5],[8,8,8,11],[2,1,2,5],[4,4,5,4],[4,5,5,5],[8,4,9,4],[8,5,9,5]]}
["※①自然調節方式により調整地容量を概算する場合に入力してください"]
[]
[null,"入　力　条　件"]
[]
[null,null,"行為後ピーク流入量",null,{"$f":"MAX('02流出計算（QT-Sグラフ）'!$J$5:$J$149)","v":0},"m3/s"]
[null,null,"（浸透考慮後）"]
[]
[null,"調整池諸元"]
[null,null,"許容放流量",null,{"$f":"MAX('01流出計算（Q-Tグラフ）'!$I$5:$I$149)","v":0},"m3/s",null,null,"概　算　結　果"]
[null,null,"（行為前ピーク流入量）"]
[null,null,null,null,null,null,null,null,null,"必要容量",370,"m3/ha"]
[null,null,"調整池高",null,null,"m"]
[]
[null,"浸透施設条件",null,{"$f":"IF('02流出計算（QT-Sグラフ）'!$B$5=1,\"浸透施設なし\",IF('02流出計算（QT-Sグラフ）'!$B$5=2,\"浸透施設あり\",\"浸透施設あり（貯留浸透モデル_道路管理者用）\"))","v":"浸透施設なし"},null,null,{"$f":"'02流出計算（QT-Sグラフ）'!$B$5","v":1},null,null,"オリフィス径（円管、直径）",0,"m"]

{"sheet":"04-①調節計算（自然調節方式）","index":8,"n_rows":57,"n_cols":26,"rows_kept":57,"cut":false,"hidden":false,"merged":[[28,15,29,18],[31,15,31,18],[1,1,1,13],[15,15,15,16],[17,15,17,16],[20,15,20,16],[22,15,22,16],[3,20,3,25],[24,15,24,16],[3,1,3,8],[5,12,6,12],[5,13,6,13],[8,12,9,12],[8,13,9,13],[3,10,3,13],[13,15,13,16],[10,15,11,18]]}
[]
[null,"入　力　条　件"]
[]
[null,"設 定 調 整 池 諸 元",null,null,null,null,null,null,null,null,"行 為 後 流 入 量",null,null,null,null,null,null,null,null,null,"計　算　結　果　（時　系　列）"]
[]
[null,"水深-容量",null,null,null,null,"放流口形状",null,null,null,"行為後ピーク流入量",null,{"$f":"MAX('02流出計算（QT-Sグラフ）'!$J$5:$J$149)","v":0},"m3/s",null,null,null,null,null,null,"時刻","行為後流入量","浸透考慮後流入量","許容放流量","調節後放流量","調整池水位"]
[null,"No","水深H（m）","容量V（m3）",null,null,"（口径）",null,null,null,"（浸透考慮後）"]
[null,1,0,0,null,1]
[null,2,null,null,null,null,"直径",0.11,"m",null,"許容放流量",null,{"$f":"MAX('01流出計算（Q-Tグラフ）'!$I$5:$I$149)","v":0},"m3/s"]
[null,3,null,null,null,null,null,null,null,null,"（行為前ピーク流入量）"]
[null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,"計　算　結　果"]
[null,5,null,null,null,null,"高さ",0,"m"]
[null,6,null,null,null,null,"幅",0,"m"]
[null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,"総合評価",null,"O.K"]
[null,8,null,null,null,null,"（管底位置）"]
[null,9,null,null,null,null,"池底高から",0,"m",null,null,null,null,null,null,"放流量評価",null,"許容放流量以下"]
[null,10]
[null,11,null,null,null,null,null,null,null,null,null,null,null,null,null,"池の容量不足",null,"無"]
[null,12]
[null,13]
[null,14,null,null,null,null,null,null,null,null,null,null,null,null,null,"最大放流量",null,2.4428568159947754E-2,"m3/s"]
[null,15]
[null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,"池内最大水深",null,0.99146102751926923,"m"]
[null,17]
[null,18,null,null,null,null,null,null,null,null,null,null,null,null,null,"池内最大ボリューム",null,109.06071302711962,"m3"]
[null,19]
[null,20]
[null,21]
[null,22,null,null,null,null,null,null,null,null,null,null,null,null,null,"許 可 申 請 図 書 の 作 成"]
[null,23]
[null,24,null,null,null,null,null,null,null,null,null,null,null,null,null,"■【様式】許可申請図書の保存場所"]
[null,25,null,null,null,null,null,null,null,null,null,null,null,null,null,"C:\\【様式】許可申請図書.xls"]
[null,26]
[null,27]
[null,28]
[null,29]
[null,30]
[null,31]
[null,32]
[null,33]
[null,34]
[null,35]
[null,36]
[null,37]
[null,38]
[null,39]
[null,40]
[null,41]
[null,42]
[null,43]
[null,44]
[null,45]
[null,46]
[null,47]
[null,48]
[null,49]
[null,50]

{"sheet":"04-②調節計算（2段）","index":9,"n_rows":57,"n_cols":26,"rows_kept":57,"cut":false,"hidden":false,"merged":[[28,15,29,18],[31,15,31,18],[3,20,3,25],[26,15,26,16],[17,15,17,16],[20,15,20,16],[22,15,22,16],[24,15,24,16],[1,1,1,13],[3,1,3,8],[3,10,3,13],[5,12,6,12],[5,13,6,13],[14,10,15,11],[14,12,15,12],[14,13,15,13],[15,15,15,16],[8,10,9,11],[8,12,9,12],[8,13,9,13],[11,10,12,11],[11,12,12,12],[11,13,12,13],[13,15,13,16],[10,15,11,18]]}
[]
[null,"入　力　条　件"]
[]
[null,"設 定 調 整 池 諸 元",null,null,null,null,null,null,null,null,"行 為 後 流 入 量",null,null,null,null,null,null,null,null,null,"計　算　結　果　（時　系　列）"]
[]
[null,"水深-容量",null,null,null,null,"■上段オリフィス",null,null,null,"行為後ピーク流入量",null,{"$f":"MAX('02流出計算（QT-Sグラフ）'!$J$5:$J$149)","v":0},"m3/s",null,null,null,null,null,null,"時刻","行為後流入量","浸透考慮後流入量","許容放流量","調節後放流量","調整池水位"]
[null,"No","水深H（m）","容量V（m3）",null,null,"放流口形状",null,null,null,"（浸透考慮後）"]
[null,1,0,0,null,1,"（口径）"]
[null,2,null,null,null,null,null,null,null,null,"許容放流量（計）",null,{"$f":"MAX('01流出計算（Q-Tグラフ）'!$I$5:$I$149)","v":0},"m3/s"]
[null,3,null,null,null,null,"直径",0.1,"m"]
[null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,"計　算　結　果"]
[null,5,null,null,null,null,null,null,null,null,"許容放流量（上段）",null,null,"m3/s"]
[null,6,null,null,null,null,"高さ",null,"m"]
[null,7,null,null,null,null,"幅",null,"m",null,null,null,null,null,null,"総合評価",null,"O.K"]
[null,8,null,null,null,null,null,null,null,null,"許容放流量（下段）",null,{"$f":"M9-M12","v":0},"m3/s"]
[null,9,null,null,null,null,"（管底位置）",null,null,null,null,null,null,null,null,"放流量評価",null,"許容放流量以下"]
[null,10,null,null,null,null,"池底高から",1,"m"]
[null,11,null,null,null,null,null,null,null,null,null,null,null,null,null,"池の容量不足",null,"無"]
[null,12,null,null,null,null,"■下段オリフィス"]
[null,13,null,null,null,null,"放流口形状"]
[null,14,null,null,null,null,"（口径）",null,null,null,null,null,null,null,null,"最大放流量（上段+下段）",null,2.4454520287668694E-3,"m3/s"]
[null,15,null,null,null,2]
[null,16,null,null,null,null,"直径",null,"m",null,null,null,null,null,null,"最大放流量（下段）",null,2.4454520287668694E-3,"m3/s"]
[null,17]
[null,18,null,null,null,null,null,null,null,null,null,null,null,null,null,"池内最大水深",null,0.85246185640973493,"m"]
[null,19,null,null,null,null,"高さ",0.01,"m"]
[null,20,null,null,null,null,"幅",0.1,"m",null,null,null,null,null,null,"池内最大ボリューム",null,85.246185640973493,"m3"]
[null,21]
[null,22,null,null,null,null,"（管底位置）",null,null,null,null,null,null,null,null,"許 可 申 請 図 書 の 作 成"]
[null,23,null,null,null,null,"池底高から",0,"m"]
[null,24,null,null,null,null,null,null,null,null,null,null,null,null,null,"■申請図書様式の保存場所"]
[null,25,null,null,null,null,null,null,null,null,null,null,null,null,null,"C:\\【様式】許可申請図書.xls"]
[null,26]
[null,27]
[null,28]
[null,29]
[null,30]
[null,31]
[null,32]
[null,33]
[null,34]
[null,35]
[null,36]
[null,37]
[null,38]
[null,39]
[null,40]
[null,41]
[null,42]
[null,43]
[null,44]
[null,45]
[null,46]
[null,47]
[null,48]
[null,49]
[null,50]

{"sheet":"04-③調節計算（ポンプ）","index":10,"n_rows":57,"n_cols":26,"rows_kept":57,"cut":false,"hidden":false,"merged":[[31,15,31,18],[22,15,22,16],[28,15,29,18],[14,11,15,11],[3,20,3,25],[13,15,13,16],[15,15,15,16],[17,15,17,16],[14,12,15,12],[24,15,24,16],[10,15,11,18],[20,15,20,16],[11,9,12,10],[11,11,12,11],[11,12,12,12],[14,9,15,10],[1,1,1,12],[3,9,3,12],[5,11,6,11],[5,12,6,12],[8,11,9,11],[8,12,9,12],[3,1,3,3],[3,5,3,7]]}
[]
[null,"入　力　条　件"]
[]
[null,"設 定 調 整 池 諸 元",null,null,null,"放 流 ポ ン プ 諸 元",null,null,null,"行 為 後 流 入 量",null,null,null,null,null,null,null,null,null,null,"計　算　結　果　（時　系　列）"]
[]
[null,"水深-容量",null,null,null,"水深-ポンプ",null,null,null,"行為後ピーク流入量",null,{"$f":"MAX('02流出計算（QT-Sグラフ）'!$J$5:$J$149)","v":0},"m3/s",null,null,null,null,null,null,null,"時刻","行為後流入量","浸透考慮後流入量","許容放流量","調節後放流量","調整池水位"]
[null,"No","水深H（m）","容量V（m3）",null,"No","水深H（m）","ポンプ規模Q(m3/s)",null,"（浸透考慮後）"]
[null,1,0,0,null,1,0,0]
[null,2,null,null,null,2,null,null,null,"許容放流量",null,{"$f":"MAX('01流出計算（Q-Tグラフ）'!$I$5:$I$149)","v":0},"m3/s"]
[null,3,null,null,null,3,null,null,null,"（行為前ピーク流入量）"]
[null,4,null,null,null,4,null,null,null,null,null,null,null,null,null,"計　算　結　果"]
[null,5,null,null,null,5]
[null,6,null,null,null,6]
[null,7,null,null,null,7,null,null,null,null,null,null,null,null,null,"総合評価",null,"O.K"]
[null,8,null,null,null,8]
[null,9,null,null,null,9,null,null,null,null,null,null,null,null,null,"放流量評価",null,"許容放流量以下"]
[null,10,null,null,null,10]
[null,11,null,null,null,11,null,null,null,null,null,null,null,null,null,"池の容量不足",null,"無"]
[null,12,null,null,null,12]
[null,13,null,null,null,13]
[null,14,null,null,null,14,null,null,null,null,null,null,null,null,null,"最大放流量",null,9.7851562499999996E-3,"m3/s"]
[null,15,null,null,null,15]
[null,16,null,null,null,16,null,null,null,null,null,null,null,null,null,"池内最大水深",null,1.9570632876203276,"m"]
[null,17,null,null,null,17]
[null,18,null,null,null,18,null,null,null,null,null,null,null,null,null,"池内最大ボリューム",null,58.711898628609823,"m3"]
[null,19,null,null,null,19]
[null,20,null,null,null,20]
[null,21,null,null,null,21]
[null,22,null,null,null,22,null,null,null,null,null,null,null,null,null,"許 可 申 請 図 書 の 作 成"]
[null,23,null,null,null,23]
[null,24,null,null,null,24,null,null,null,null,null,null,null,null,null,"■申請図書様式の保存場所"]
[null,25,null,null,null,25,null,null,null,null,null,null,null,null,null,"C:\\【様式】許可申請図書.xls"]
[null,26,null,null,null,26]
[null,27,null,null,null,27]
[null,28,null,null,null,28]
[null,29,null,null,null,29]
[null,30,null,null,null,30]
[null,31,null,null,null,31]
[null,32,null,null,null,32]
[null,33,null,null,null,33]
[null,34,null,null,null,34]
[null,35,null,null,null,35]
[null,36,null,null,null,36]
[null,37,null,null,null,37]
[null,38,null,null,null,38]
[null,39,null,null,null,39]
[null,40,null,null,null,40]
[null,41,null,null,null,41]
[null,42,null,null,null,42]
[null,43,null,null,null,43]
[null,44,null,null,null,44]
[null,45,null,null,null,45]
[null,46,null,null,null,46]
[null,47,null,null,null,47]
[null,48,null,null,null,48]
[null,49,null,null,null,49]
[null,50,null,null,null,50]